
[MINI UPS SYSTEM](http://engg-project2.blogspot.com/2010/07/mini-ups-system.html)

             This circuit provides an uninterrupted power supply (UPS)  
to operate 12V, 9V and 5V DC-powered instruments at up to 1A  
current. The backup battery takes up the load without spikes or delay when  
the mains power gets interrupted. It can also be used as a workbench power  
supply that provides 12V, 9V and 5V operating voltages.  
The circuit immediately disconnects the load when  
the battery voltage reduces to 10.5V to prevent deep discharge of the battery.  
LED1 indication is provided to show the full charge voltage level of the battery.  
Miniature white LEDs (LED2 and LED3) are used as emergency lamps  
during power failure at night.



Apparatus required for this are:

* Variable transformer
* Diode
* SCR or transistor
* Battery
* Zener diode
* ON/OFF switch
* Resistance & Capacitor
* IC: IC7809 ,IC7805

            A standard step-down transformer provides 12V of AC, which  
is rectified by diodes D1 and D2. Capacitor C1 provides ripple-free DC to  
charge the battery and to the remaining circuit.   
When the mains power is on, diode D3 gets forward biased to  
charge the battery. Resistor R1 limits the charging current, Potentiometer  
VR1 (10k) with transistor T1 acts as the voltage comparator to indicate  
the voltage level. VR1 is so adjusted that LED1 is in the ‘off’ mode, when the battery is fully charged, LED1 glows indicating a full voltage level  
of 12V.  
  
           When the mains power fails, diode D3 gets reverse biased and  
D4 gets forward biased so that the battery can automatically take up  
the load without any delay. When the battery voltage or input voltage  
falls below 10.5V, a cut-off circuit is used to prevent deep discharging of  
the battery. Resistor R3, zener diode ZD1 (10.5V) and transistor T2 form  
the cut-off circuit. When the voltage level is above 10.5V, transistor  
T2 conducts and its base becomes negative (as set by R3, VR2 and ZD1).  
But when the voltage reduces below 10.5V, the zener diode stops conduction  
and the base voltage of transistor T2 becomes positive. It goes into  
the ‘cut-off’ mode and prevents the current in the output stage. Preset  
VR2 (22k) adjusts the voltage below 0.6V to make T2 work if the voltage  
is above 10.5V.

            When power from the mains is available, all output voltages—12V,  
9V and 5V—are ready to run the load. On the other hand, when the  
mains power is down, output voltages can run the load only when the  
battery is fully charged (as indicated by LED1). For the partially charged  
battery, only 9V and 5V are available. Also, no output is available when the  
voltage goes below 10.5V. If battery voltage varies between 10.5V and  
13V, output at terminal A may also vary between 10.5V and 12V, when  
the UPS system is in battery mode.

   
            Outputs at points B and C provide 9V and 5V, respectively, through regulator  
ICs (IC1 and IC2), while output A provides 12V through the zener  
diode. The emergency lamp uses two ultra-bright white LEDs (LED2 and  
LED3) with current limiting resistors R5 and R6. The lamp can be manually  
switched ‘on’ and ‘off’ by S1. the circuit is assembled on a general-  
purpose PCB. There is adequate space between the components to  
avoid overlapping. heat sinks for transistor T2 and regulator ICs (7809 and  
7805) to dissipate heat are used. The positive and negative rails  
should be strong enough to handle high current. Before connecting the  
circuit to the battery and transformer, connect it to a variable power supply.  
Provide 12V DC and adjust VR1 till LED1 glows. After setting the high  
voltage level, reduce the voltage to 10.5V and adjust VR2 till the output  
trips off. After the settings are complete, remove the variable power supply  
and connect a fully-charged battery to the terminals and see that LED1 is  
on. After making all the adjustments connect the circuit to the battery and  
transformer. The battery used in the circuit is a 12V, 4.5Ah UPS battery.